AXIS M4317-PLR Panoramic Camera
Optimized for surveillance onboard buses, this discreet, panoramic camera is designed to withstand shock and vibrations. It delivers a complete 180° or 360° overview for total situational awareness. Thanks to built-in IR illumination with individually controllable LEDs, it ensures clear, reflection-free footage and excellent image quality even in low light or complete darkness. Delivered factory-focused, it includes digital roll functionality to remotely adjust the rotation of the camera overview. Furthermore, this high-performance camera includes built-in cybersecurity features to help prevent unauthorized access and safeguard your system. Plus, it supports advanced analytics based on deep learning on the edge.
• Complies with industry bus regulations
• Sharpdome technology
• Complete 180° and 360° overview
• Built-in IR with individual IR LEDs
• Built-in cybersecurity features

The contractor or designated subcontractor shall submit credentials of completed manufacturer certification, verified by a third party organization, as proof of the knowledge.
The main unit shall be manufactured by a company that have signed and support the UN Global Compact initiative as defined by United Nations www.unglobalcompact.org/

Image sensor
1/1.8” progressive scan RGB CMOS
Lens
Focal length: 1.1 mm, F2.2
Horizontal field of view: 182°
Vertical field of view: 182°
Fixed iris, IR corrected, fixed focus
Day and night
Automatic IR-cut filter
Minimum illumination
Color: 0.16 lux at 50 IRE, F2.2
B/W: 0.03 lux at 50 IRE, F2.2
0 lux with IR illumination on
Shutter speed
1/33500 s to 0.2 s
Camera angle adjustment
Digital roll: ± 180°
System on Chip model
Manufacturer’s own chipset (8th gen)
Memory
2048 MB RAM, 8192 MB Flash
Compute capabilities
Deep learning processing unit (DLPU)
Video compression
H.264 (MPEG-4 Part 10/AVC) Baseline, Main and High Profiles
H.265 (MPEG-H Part 2/HEVC) Main Profile
Motion JPEG
Resolution
Overview: 2160x2160 to 160x160
Panorama: 2560x1440 to 192x72
Double Panorama: 2560x1920 to 384x288
Quad view: 2560x1920 to 384x288
View area 1-4: 1920x1440 to 256x144
Corner right and left: 2368x1184 to 192x72
Double corner: 2016x2016 to 384x288
Corridor: 2560x1920 to 256x144
Frame rate
Up to 25/30 fps (60/50 Hz) in all resolutions
360° overview up to 2160x2160 without WDR: 50/60 fps @(50/60 Hz)
360° overview and dewarped views up to max resolution with WDR: up to 25/20 fps @(50/60 Hz)
Video streaming
Multiple, individually configurable streams in H.264, H.265 and Motion JPEG

Controllable frame rate and bandwidth
VBR/ABR/MBR H.264/H.265
Video streaming indicator
WDR
advanced WDR imaging technology: Up to 120 dB depending on scene
Noise reduction
Spatial filter (2D noise reduction)
Temporal filter (3D noise reduction)
Image settings
Saturation, contrast, brightness, sharpness, local contrast, tone mapping, white balance, day/night threshold, exposure mode, exposure zones, compression, mirroring, dynamic text and image overlay, polygon privacy mask
Pan/Tilt/Zoom
Digital PTZ of view areas, digital PT of panorama, corner, corridor and quad views, preset positions, guard tours
Audio features
Network speaker pairing
Audio input/output
Two-way audio connectivity via portcast technology
Network protocols
IPv4, IPv6 USGv6, ICMPv4/ICMPv6, HTTP, HTTPS, HTTP/2, TLS, QoS Layer 3 DiffServ, FTP, SFTP, CIFS/SMB, SMTP, mDNS (Bonjour), UPnP®, SNMP v1/v2c/v3 (MIB-II), DNS/DNSv6, DDNS, NTP, NTS, RTSP, RTP, SRTP/RTSPS, TCP, UDP, IGMPv1/v2/v3, RTCP, DHCPv4/v6, SSH, LLDP, CDP, MQTT v3.1.1, Syslog, Link-Local address (ZeroConf), IEEE 802.1X (EAP-TLS), IEEE 802.1AR
Application Programming Interface
Open API for software integration.. application includes Native SDK and Computer Vision SDK.

ONVIF® Profile G, ONVIF® Profile M, ONVIF® Profile S, and ONVIF® Profile T, specification at onvif.org
Support for Session Initiation Protocol (SIP) for integration with Voice over IP (VoIP) systems, peer to peer or integrated with SIP/PBX.
Onscreen controls
Privacy masks
IR illumination
Media clip
Event conditions
Device status: above operating temperature, above or below operating temperature, below operating temperature, casing open, IP address removed, live stream active, network lost, new IP address, system ready, within operating temperature
Edge storage: recording ongoing, storage disruption, storage health issues detected
I/O: digital input is active, digital output is active, manual trigger, virtual input is active
MQTT: stateless
Scheduled and recurring: schedule
Video: average bitrate degradation, day-night mode, tampering
Event actions
Day-night mode: use while the rule is active
I/O: toggle once, toggle while the rule is active
Illumination: use lights, use lights while the rule is active
Images: FTP, HTTP, HTTPS, SFTP, email and network share
MQTT: publish
Notification: HTTP, HTTPS, TCP and email
Overlay text: use, use while the rule is active
Recordings: record video, record video while the rule is active
SNMP trap messages: send, send while the rule is active
Status LED: flash, flash while the rule is active
Video clips: FTP, HTTP, HTTPS, SFTP, email and network share
WDR mode: set, set while the rule is active
Built-in installation aids
Pixel counter, level grid, digital roll
Object Analytics
Object classes: humans, vehicles (types: cars, buses, trucks, bikes)
Trigger conditions: line crossing, object in area
Up to 10 scenarios
Metadata visualized with trajectories and color-coded bounding boxes
Polygon include/exclude areas
ONVIF Motion Alarm event
Metadata
Object data: Classes: humans, faces, vehicles (types: cars, buses, trucks, bikes)
Confidence, position
Event data: Producer reference, scenarios, trigger conditions
Applications
Included
object analytics, video motion detection, active tampering alarm
Supported
people counter
Support for enabling installation of third-party applications
Product markings
CSA, UL/cUL, BIS, UKCA, CE, KC
Supply chain
TAA compliant
EMC
ECE R10 rev.06, EN 55035, EN 55032 Class A, EN 50121-4, EN 61000-6-1, EN 61000-6-2, EN 61547
Australia/New Zealand: RCM AS/NZS CISPR 32 Class A
Canada: ICES-3(A)/NMB-3(A)
Japan: VCCI Class A
Korea: KS C 9835, KS C 9832 Class A
USA: FCC Part 15 Subpart B Class A
Railway: IEC 62236-4
Safety
IEC/EN/UL 62368-1 ed. 3, CAN/CSA C22.2 No. 62368-1 ed. 3, IEC/EN 62471 risk group exempt, UN ECE R118
Environment
IEC 60068-2-1, IEC 60068-2-2, IEC 60068-2-6, IEC 60068-2-14, IEC 60068-2-27, IEC 60068-2-78, IEC TR 60721-4-5 Class 5M3 (Vibration, Shock), IEC/EN 62262 IK10, IEC/EN 60529 IP66, ISO 4892-2, NEMA 250 Type 4X, NEMA TS 2 (2.2.7-2.2.9), EN 50155, IEC/EN 61373 Category 1 Class B, ISO 21207 (Method B)
Network
NIST SP500-267
Edge security
Software: Signed firmware, brute force delay protection, digest authentication, password protection, AES-XTS-Plain64 256bit SD card encryption
Hardware: Secure boot, cryptographic compute module with Manufacturer's device ID, signed video, secure keystore (CC EAL4+ certified hardware protection of cryptographic operations and keys)
Network security
IEEE 802.1X (EAP-TLS), IEEE 802.1AR, HTTPS/HSTS, TLS v1.2/v1.3, Network Time Security (NTS), X.509 Certificate PKI, IP address filtering
Casing
IP66-, NEMA 4X- and IK10-rated
Polycarbonate hard-coated dome
Aluminum
Color: white NCS S 1002-B
Repaintable skin cover accessory
Mounting
Mounting bracket with junction box holes (double-gang, single-gang, and 4” octagon)
¼”-20 UNC tripod screw thread
Power
Power over Ethernet (PoE) IEEE 802.3af/802.3at Type 1 Class 3
Typical 5.7 W, max 12.95 W
Connectors
Network: Shielded RJ45 10BASE-T/100BASE-TX PoE
I/O: Terminal block for 1 supervised alarm input and 1 output (12 VDC output, max. load 25 mA)
Audio: Audio and I/O connectivity via portcast technology
IR illumination
IR with power-efficient, long-life 850 nm IR LEDs
Range of reach 20 m (65.6 ft) depending on the scene
Storage
Support for microSD/microSDHC/microSDXC card
Recording to network-attached storage (NAS)
For SD card and NAS recommendations, refer to the manufacturer's webpage
Operating conditions
-40 °C to 50 °C (-40 °F to 122 °F)
Start-up temperature: -30 °C
Humidity 10-100% RH (condensing)
Storage conditions
-40 °C to 65 °C (-40 °F to 149 °F)
Humidity 5-95% RH (non-condensing)
Dimensions
Height: 70 mm (2.7 in)
ø 149 mm (5.9 in)
Effective Projected Area (EPA): 0.0076 m2 (0.025 ft2)
Weight
860 g (1.9 lb)
Box content
Camera, installation guide, terminal block connector, connector guard, cable gaskets, cable hole lid, owner authentication key
Languages
English, German, French, Spanish, Italian, Russian, Simplified Chinese, Japanese, Korean, Portuguese, Polish, Traditional Chinese
Warranty
5-year warranty
Substance control
PVC free, BFR/CFR free in accordance with JEDEC/ECA Standard JS709
RoHS in accordance with EU RoHS Directive 2011/65/EU/ and EN 63000:2018
REACH in accordance with (EC) No 1907/2006.
Materials
Renewable carbon-based plastic content: 29.6% (bio-based)
Screened for conflict minerals in accordance with OECD guidelines
Environmental responsibility
/environmental-responsibility
The manufacturer is a signatory of the UN Global Compact, read more at unglobalcompact.org
Key features and technologies
Artificial intelligence (AI)
The AI functionality should detect and classify both persons and vehicles. The configuration menu of the device should make it possible to detect only persons, only vehicles, or both. 
The AI functionality to detect and classify persons and vehicles is configured by the manufacturer and is based on Deep Learning principles. 
The device that provides the AI functionality should make the functionality available directly, without requiring additional device applications. 
The detected objects should be highlighted with red frames for persons and blue frames for vehicles, including an indication icon of the classification.
Built-in cybersecurity
Cryptographic compute module is a secure cryptographic compute module (secure module or secure element) in which the Manufacturer's device ID is securely and permanently installed and stored.
Signed firmware is implemented by the software vendor signing the firmware image with a private key, which is secret. When firmware has this signature attached to it, a device will validate the firmware before accepting and installing it. If the device detects that the firmware integrity is compromised, it will reject the firmware upgrade. Signed firmware is based on the industry-accepted RSA public-key encryption method.
Secure boot is a boot process that consists of an unbroken chain of cryptographically validated software, starting in immutable memory (boot ROM). Being based on signed firmware, secure boot ensures that a device can boot only with authorized firmware. Secure boot guarantees that the Manufacturer's device is completely clean from possible malware after resetting to factory default.
TPM is short for Trusted Platform Module. A TPM is a component that provides a set of cryptographic features suitable for protecting information from unauthorized access. The private key is stored in the TPM and never leaves the TPM. All cryptographic operations requiring the use of the private key are sent to the TPM to be processed. This ensures that the secret part of the certificate remains safe even in the event of a security breach.
Advanced low-light technology
Advanced low-light technology must give a network camera extreme light sensitivity, so that the camera remains in day mode and continues to deliver images in color. In surveillance situations, color may be the critical factor that enables identification of a person, an object, or a vehicle. 
A camera with advanced low-light technology must be able to use shorter exposure times, to keep blur and noise to a minimum.
Advanced low-light technology should combine high-quality lenses and image sensors optimized for surveillance, with digital image processing algorithms embedded in the system-on-chip. 
The camera must be equipped with built-in IR LEDs.
The camera features technology that dynamically adapts the range and strength of the infrared light to the camera's zoom range.
The infrared technology features a mechanism that automatically and dynamically controls the amount of infrared light, ensuring that the entire field-of-view is illuminated proportionally, providing a high-quality and uniformly illuminated camera image, while suppressing noise. 
The IR LEDs will emit light at a wavelength of 850 nm.
The camera supporting the infrared technology must be powered via PoE.
Video compression technology
The video compression technology must make it possible to use higher resolutions and so increase forensic usability, while also reducing storage costs. 
The video compression technology must be a standards-compatible video encoder implementation that lowers bandwidth and storage requirements by an average of 50% or more when compared to standard methods. 
Important details and motion should be preserved at high quality, while the rest of the image information should be filtered more aggressively, to make optimal use of the available bandwidth. 
The technology consists of a collection of algorithms that analyze the video stream in real time: 
• Dynamic ROI (regions of interest) - identifies regions of interest based on objects, people or motion in the scene, and applies the correct level of compression from a forensic perspective.
• Dynamic GOP (group of pictures) - the camera sends bandwidth-heavy I-frames less frequently when there is no motion in the scene.
• Dynamic FPS (frames per second) - reduces the bitrate when there is little or no motion in the scene. The camera captures and analyses video at full frame rate, but unnecessary frames are not encoded. 

The video compression technology should include support for PTZ camera functionality, 4K Ultra HD, multi-megapixel cameras and 360-degree panoramic cameras, dynamic FPS limitation and dynamic FPS frame skipping. 
The video compression technology should provide support for H.264 in all products, as well as additional support for H.265 in selected products, to enable flexible migration over an extended period.