AXIS D1110 Video Decoder 4K
This 4K video decoder can be used to display live video in sequence view, and up to 8 video streams in multiview. It offers a cost-effective solution for video monitoring where live video can be displayed without the use of a PC. It can be used with monitors that support HDMI, plus, it can display advertisements or general information with or without audio. Furthermore, it supports both PoE and DC power for fast and easy installation.
• 4K video with HDMI output
• PoE or DC powered
• Audio out
• Seamless sequencing and multiview
• Intuitive interface

The contractor or designated subcontractor shall submit credentials of completed manufacturer certification, verified by a third party organization, as proof of the knowledge.
The main unit shall be manufactured by a company that have signed and support the UN Global Compact initiative as defined by United Nations www.unglobalcompact.org/

System on Chip model
i.MX8 QuadPlus
Memory
2 GB RAM, 1 GB Flash
Video compression
H.264/AVC (MPEG-4 Part 10/AVC Baseline, Main and High profile (B-frame and interlaced rendering are not supported))
H.265/HEVC Main profile
Frame rate
Up to 60 fps depending on resolution
Video streaming
Up to eight streams in VPU (Video Processing Unit)
Video output
All formats 16:9:
UHD
3840x2160 @25/30 fps (50/60 Hz)
FHD 1080p
1920x1080 @50/60 fps (50/60 Hz)
1920x1080 @25/30 fps (50/60 Hz)
HD 720p
1280x720 @50/60 fps (50/60 Hz)
SD
720x576 @50 fps (50 Hz)
720x480 @60 fps (60 Hz)
Audio output
Line output, HDMI (stereo)
Network protocols
IPv4, IPv6 USGv6, ICMPv4/ICMPv6, HTTP, HTTPS, HTTP/2, TLS, CIFS/SMB, SMTP, mDNS (Bonjour), UPnP®, SNMP, v1/v2c/v3 (MIB-II), DNS/DNSv6, DDNS, NTP, NTS, RTSP, RTP, RTSPS, TCP, UDP, IGMPv1/v2/v3, RTCP, DHCPv4/v6, SSH, LLDP, CDP, MQTT v3.1.1, Syslog, Link-Local address (ZeroConf), IEEE 802.1X (EAP-TLS), IEEE 802.1AR
Application Programming Interface
Open API for software integration., ; specifications at /developer-community. application includes Native SDK
Event conditions
IP address removed, live stream active, network lost, new IP address, system ready
Edge storage: storage disruption, storage health issues detected
I/O: manual trigger, virtual input
MQTT: stateless
Scheduled and recurring: schedule
Event actions
MQTT: publish
Notification: HTTP, HTTPS, TCP and email
SNMP traps: send, send while the rule is active
Status LED: flash, flash while the rule is active
Product markings
UL/cUL, UKCA, CE, KC, VCCI, RCM
Supply chain
TAA compliant
EMC
CISPR 35, CISPR 32 Class A, EN 55035, EN 55032 Class A, EN 61000-3-2, EN 61000-3-3, EN 61000-6-1, EN 61000-6-2
Australia/New Zealand: RCM AS/NZS CISPR 32 Class A
Canada: ICES-3(A)/NMB-3(A)
Japan: VCCI Class A
Korea: KS C 9835, KS C 9832 Class A
USA: FCC Part 15 Subpart B Class A
Safety
IEC/EN/UL 62368-1 ed. 3, CAN/CSA C22.2 No. 62368-1 ed. 3
Environment
IEC 60068-2-1, IEC 60068-2-2, IEC 60068-2-6, IEC 60068-2-14, IEC 60068-2-27, IEC 60068-2-78, IEC/EN 60529 IP30
Network
NIST SP500-267
Edge security
Software: Signed firmware, brute force delay protection, digest authentication, password protection
Hardware: cryptographic compute module cybersecurity platform
Secure element (CC EAL 6+), Manufacturer's device ID, secure keystore, secure boot
Network security
IEEE 802.1X (EAP-TLS), IEEE 802.1AR, HTTPS/HSTS, TLS v1.2/v1.3, Network Time Security (NTS), X.509 Certificate PKI, IP address filtering
Casing
IP30-rated
Aluminum casing
Color: NCS S 9000-N
Security slot
Mounting
manufacturer T91A03 DIN Rail Clip A, mounting bracket, compatible with VESA mounting hole patterns
Power
Power over Ethernet (PoE) IEEE 802.3af/802.3at Type 2 Class 4
10–28 V DC, max 17 W
Connectors
Network: RJ45 10BASE-T/100BASE-TX/1000BASE-T PoE
Audio: 3.5 mm line out, stereo
Power: DC input, terminal block
2x USB type A
SD-card slot (Highspeed/UHS-1)
HDMI type A, CEC supported
Storage
Support for microSD/microSDHC/microSD UHS-1 card
Operating conditions
0 °C to 40 °C (32 °F to 104 °F)
Humidity 10–85% RH (non-condensing)
Storage conditions
-20 °C to 65 °C (-4 °F to 149 °F)
Humidity 5–95% RH (non-condensing)
Dimensions
For the overall product dimensions, see the dimension drawing in this datasheet
Weight
500 g (1.10 lb)
Box content
Video decoder, installation guide, terminal block connector
Languages
English, German, French, Spanish, Italian, Russian, Simplified Chinese, Japanese, Korean, Portuguese, Polish, Traditional Chinese, Dutch, Czech, Swedish, Finnish, Turkish, Thai, Vietnamese
Warranty
5-year warranty
Substance control
RoHS in accordance with EU RoHS Directive 2011/65/EU/ and EN 63000:2018
REACH in accordance with (EC) No 1907/2006. For SCIP UUID, see echa.europa.eu
Materials
Screened for conflict minerals in accordance with OECD guidelines
Environmental responsibility

The manufacturer is a signatory of the UN Global Compact, read more at unglobalcompact.org