AXIS P5654-E PTZ Network Camera
This network camera is a cost-effective, high performance PTZ camera that offers wide area coverage with 77° field of view. It features advanced low-light technology to capture low-light images with more saturated colors and sharper images of moving objects and, advanced WDR imaging for clarity even when there’s both dark and light areas in the scene. Electronic image stabilization for stable images and enhanced security features including signed firmware and secure boot. With IP66, NEMA 4X and IK10 ratings it’s resistant to both harsh weather conditions and impacts. Plus, you get extended capabilities for advanced analytics.
• HDTV 720p with 21x optical zoom
• Advanced low-light technology and WDR imaging 
• Signed firmware and secure boot
• Electronic image stabilization
• Built-in reduced bandwidth and storage technology with support for H.264 and H.265

The product, including all its components, shall not contain any added PVC.
The contractor or designated subcontractor shall submit credentials of completed manufacturer certification, verified by a third party organization, as proof of the knowledge.
The main unit shall be manufactured by a company that have signed and support the UN Global Compact initiative as defined by United Nations www.unglobalcompact.org/

Image sensor
1/2.8” progressive scan RGB CMOS
Lens
Varifocal, 4.0-84.6 mm, F1.6 - 4.5
Horizontal field of view: 77.0°- 3.6°
Vertical field of view: 43.1°- 2.0°
Autofocus and auto-iris
Day and night
Automatically removable infrared-cut filter
Minimum illumination
Color: 0.11 lux at 50 IRE F1.6
Color: 0.1 lux at 30 IRE F1.6
B/W: 0.03 lux at 50 IRE F1.6
B/W: 0.01 lux at 30 IRE F1.6
Shutter speed
1/66500 s to 2 s
Pan/Tilt/Zoom
Pan: 360° endless, 0.1°- 350°/s
Tilt: 180°, 0.1°- 350°/s
Zoom: 21x optical, 12x digital, Total 252x zoom
256 preset positions, e-flip, limited guard tour, control queue, on-screen directional indicator, set new pan 0°, focus window, focus recall
System on Chip model
Manufacturer’s own chipset (7th gen)
Memory
1024 MB RAM, 512 MB Flash
Compute capabilities
Machine learning processing unit (MLPU)
Video compression
H.264 (MPEG-4 Part 10/AVC) Baseline, Main and High Profiles
H.265 (MPEG-H Part 2/HEVC) Main Profile
Motion JPEG
Resolution
1280x720 HDTV 720p to 320x180
Frame rate
Up to 60/50 fps (60/50 Hz) in all resolutions
Video streaming
Multiple, individually configurable streams in H.264, H.265 and Motion JPEG
Controllable frame rate and bandwidth

VBR/ABR/MBR H.264/H.265
Low latency mode
Image settings
Compression, saturation, brightness, sharpness, contrast, local contrast, white balance, exposure control, exposure zones, advanced WDR imaging technology: Up to 120 dB depending on scene, defogging, day/night shift level, tone mapping, fine tuning of low-light behavior, rotation: 0°, 180°, text and image overlay, image freeze on PTZ, electronic image stabilization, scene profiles, 20 individual polygon privacy masks
Security
IP address filtering, HTTPS encryption, IEEE 802.1X (EAP-TLS) network access control, user access log, centralized certificate management
Network protocols
IPv4, IPv6 USGv6, ICMPv4/ICMPv6, HTTP, HTTP/2, HTTPS, TLS, QoS Layer 3 DiffServ, FTP, SFTP, CIFS/SMB, SMTP, mDNS (Bonjour), UPnP®, SNMP v1/v2c/v3 (MIB-II), DNS/DNSv6, DDNS, NTP, NTS, RTSP, RTP, SRTP/RTSPS, TCP, UDP, IGMPv1/v2/v3, RTCP, ICMP, DHCPv4/v6, ARP, SSH, NTCIP, LLDP, CDP, MQTT v3.1.1, Secure syslog (RFC 3164/5424, UDP/TCP/TLS), Link-Local address (ZeroConf)
Application Programming Interface
Open API for software integration.

ONVIF® Profile G, ONVIF® Profile M, ONVIF® Profile S, and ONVIF® Profile T, specification at onvif.org
Event conditions
Device status: Above operating temperature, Above or below operating temperature, Below operating temperature, Fan failure, IP address removed, Network lost, New IP address, Shock detected, Storage failure, System ready, Within operating temperature, Edge storage, Recording ongoing, Storage disruption
I/O: Manual trigger, Virtual input
PTZ: PTZ malfunctioning, PTZ movement: Camera 1, PTZ preset position reached: Camera 1, PTZ ready
Scheduled and recurring: Scheduled event
Video: Day-night mode, Live stream open
Event actions
Day-night mode, go to preset position, guard tour, upload of images or video clips via FTP, SFTP, HTTP, HTTPS, network share and email, notification to email, HTTP, HTTPS, TCP and SNMP trap, overlay text, prioritized text, record video to SD card and network share, WDR mode
Built-in installation aids
Pixel counter
Object Analytics
Object classes: humans, vehicles
Trigger conditions: line crossing, object in area, time in areaBETA
Up to 10 scenarios
Metadata visualized with trajectories and color-coded bounding boxes
Polygon include/exclude areas
Perspective configuration
ONVIF Motion Alarm event
Metadata
Object data: Classes: humans, faces, vehicles, license plates
Confidence, position
Applications
Included
object analytics
video motion detection, motion guard, fence guard, loitering guard, advanced gatekeeper, autotracker 2
Support for enabling installation of third-party applications
Edge security
Software: Signed firmware, brute force delay protection, digest authentication, password protection, AES-XTS-Plain64 256bit SD card encryption
Hardware: Secure boot
Network security
IEEE 802.1X (EAP-TLS), HTTPS/HSTS, TLS v1.2/v1.3, Network Time Security (NTS), X.509 Certificate PKI, IP address filtering
Casing
IP66-, NEMA 4X- and IK10-rated
Aluminum casing, polycarbonate (PC) dome
Color: white NCS S 1002-B, repaintable skin cover
Sustainability
PVC free
Power
PoE+ midspan 1–port: 100–240 V AC, max 37 W
IEEE 802.3at, Type 2 Class 4
Camera consumption: typical 8 W, max 16 W
(PoE+ midspan not included)
Connectors
RJ45 10BASE-T/100BASE-TX PoE
RJ45 push-pull connector (IP66) included
Storage
Support for SD/SDHC/SDXC card
Support for SD card encryption (AES-XTS-Plain64 256bit)
Recording to network-attached storage (NAS)
For SD card and NAS recommendations, refer to the manufacturer's webpage
Operating conditions
-30 °C to 50 °C (-22 °F to 122 °F)
Maximum intermittent temperature 55°C
Humidity 10–100% RH (condensing)
Storage conditions
-40 °C to 65 °C (-40 °F to 149 °F)
Humidity 5–95% RH (non-condensing)
Approvals
EMC
EN 50121-4, EN 55024, EN 55032 Class A, EN 61000-3-2, EN 61000-3-3, EN 61000-6-1, EN 61000-6-2, FCC Part 15 Subpart B Class A, ICES-3(A)/NMB-3(A),IEC 62236-4, KC KN32 Class A, KC KN35, RCM AS/NZS CISPR 32 Class A, VCCI Class A
Safety
IEC/EN/UL 62368-1, IEC/EN/UL 60950-22, IS 13252
Environment
IEC 60068-2-1, IEC 60068-2-2, IEC 60068-2-6, IEC 60068-2-14,
IEC 60068-2-27, EC 60068-2-78, IEC/EN 60529 IP66, IEC/EN 62262 IK10, NEMA 250 Type 4X 
Network
NIST SP500-267, IPv6 USGv6
Dimensions
Height: 217 mm (8.54 in)
ø 188 mm (7.4 in)
Weight
2.5 kg (5.5 lb)
Languages
English, German, French, Spanish, Italian, Russian, Simplified Chinese, Japanese, Korean, Portuguese, Traditional Chinese
Warranty
5-year warranty