AXIS P3227-LV Network Camera
This network camera is a streamlined 5 MP fixed dome that features a varifocal lens with remote zoom and focus, which facilitates installation and eliminates the need for hands-on fine tuning. Equipped with advanced WDR imaging technology to handle scenes with strong variations in light, advanced low-light technology, as well as IR illumination with power-efficient bulit-in IR LED technology, this versatile camera provides exceptional video quality in any light conditions. It supports reduced bandwidth and storage needs technology that significantly reduces bandwidth and storage requirements.
• 5 MP resolution in full frame rate
• Advanced WDR imaging and low-light technology
• Power-efficient built-in IR LED technology
• Remote zoom and focus
• Reduced bandwidth and storage needs technology

The product, including all its components, shall not contain any added PVC.
The contractor or designated subcontractor shall submit credentials of completed manufacturer certification, verified by a third party organization, as proof of the knowledge.
The main unit shall be manufactured by a company that have signed and support the UN Global Compact initiative as defined by United Nations www.unglobalcompact.org/

Image sensor
Progressive scan RGB CMOS 1/2.5”
Lens
Varifocal, 3.5–10 mm, F1.7
Horizontal field of view: 100°-38°
Vertical field of view: 51°–22°
Remote zoom and focus, P-Iris control, IR corrected
Day and night
Automatically removable infrared-cut filter
Minimum illumination
Color: 0.18 lux at 50 IRE, F1.7
B/W: 0.04 lux F1.7 at 50 IRE, 0 lux with IR illumination on
Shutter speed
1/62500 s to 2 s
Camera angle adjustment
Pan ±180°, tilt -40 to +75°, rotation ±95°
System on Chip model
Manufacturer’s own chipset (6th gen)
Memory
1 GB RAM, 512 MB Flash
Video compression
H.264 (MPEG-4 Part 10/AVC) Baseline, Main and High Profiles
Motion JPEG
Resolution
3072x1728 to 160x90
Frame rate
25/30 fps with power line frequency 50/60 Hz
Video streaming
Multiple, individually configurable streams in H.264 and Motion JPEG

Controllable frame rate and bandwidth
VBR/ABR/MBR H.264
Multi-view streaming
8 individually cropped out view areas.
Pan/Tilt/Zoom
Digital PTZ, Preset positions
Image settings
Compression, Color, Brightness, Sharpness, Contrast, Local contrast, White balance, Exposure control (including automatic gain control), Exposure zones, Fine tuning of behavior at different light levels, advanced WDR imaging technology: up to 120 dB depending on scene, Text and image overlay, Mirroring of images, Privacy masks
Rotation: 0°, 90°, 180°, 270°, including corridor format
Audio input/output
Two-way audio connectivity via audio and I/O interfaces with portcast technology
Security
Password protection, IP address filtering, HTTPS encryption, IEEE 802.1X (EAP-TLS) network access control, digest authentication, user access log, centralized certificate management, brute force delay protection, signed firmware
Network protocols
IPv4, IPv6 USGv6, ICMPv4/ICMPv6, HTTP, HTTP/2, HTTPS, TLS, QoS Layer 3 DiffServ, FTP, SFTP, CIFS/SMB, SMTP, mDNS (Bonjour), UPnP, SNMP v1/v2c/v3 (MIB-II), DNS/DNSv6, DDNS, NTP, NTS, RTSP, RTP, SRTP, TCP, UDP, IGMPv1/v2/v3, RTCP, ICMP, DHCPv4/v6, ARP, SIP, SSH, LLDP, CDP, MQTT v3.1.1, Syslog, Link-Local address (ZeroConf)
Application Programming Interface
Open API for software integration. and ; specifications at

ONVIF® Profile G, ONVIF® Profile M, ONVIF® Profile S, and ONVIF® Profile T specification at onvif.org
Support for Session Initiation Protocol (SIP) for integration with Voice over IP (VoIP) systems, peer to peer or integrated with SIP/PBX
Event triggers
Analytics, edge storage events, virtual inputs through API
Event actions
Record video: SD card and network share
Upload of images or video clips: FTP, SFTP, HTTP, HTTPS, network share and email
Pre- and post-alarm video or image buffering for recording or upload
Notification: email, HTTP, HTTPS, TCP and SNMP trap
Overlay text, IR illumination on/off
Data streaming
Event data
Built-in installation aids
Remote zoom, remote focus, pixel counter
Applications
Included
motion guard, fence guard, loitering guard
video motion detection, active tampering alarm
Supported
intelligent detect and track application, AXIS Demographic Identifier
Support for additional applications if the device is used with compatible accessories. For more information, contact your distributor partner.
Support for enabling installation of third-party applications
Casing
IP52-rated, IK08 impact-resistant, polycarbonate casing with hard-coated dome and dehumidifying membrane
Encapsulated electronics and captive screws
Color: white NCS S 1002-B
Mounting
Mounting bracket with holes for junction boxes (double-gang, single-gang, and 4” octagon) and for wall or ceiling mount
¼”-20 UNC tripod screw thread
Sustainability
PVC free
Power
Power over Ethernet (PoE) IEEE 802.3af/802.3at Type 1 Class 3,
max 11.5 W, typical 8.4 W
Connectors
RJ45 10BASE-T/100BASE-TX PoE
Audio and I/O connectivity via audio and I/O interfaces with portcast technology
IR illumination
IR with power-efficient, long-life 850 nm IR LEDs. Range of reach 30 m (100 ft) or more depending on the scene
Storage
Support for microSD/microSDHC/microSDXC card
Support for SD card encryption (AES-XTS-Plain64 256bit)
Support for recording to network-attached storage (NAS)
For SD card and NAS recommendations, refer to the manufacturer's webpage
Operating conditions
0 °C to 50 °C (32 °F to 122 °F)
Humidity 10 to 85% RH (non-condensing)
Storage conditions
-40 °C to 65 °C (-40 °F to 149 °F)
Humidity 5-95% RH (non-condensing)
Approvals
EMC
EN 55032 Class B, EN 50121-4, IEC 62236-4, EN 55024, EN 61000-6-1, EN 61000-6-2, FCC Part 15 Subpart B Class A and B, ICES-003 Class B, VCCI Class B, RCM AS/NZS CISPR 22 Class B, KCC KN32 Class B, KN35
Safety
IEC/EN/UL 60950-1, IEC/EN 62471, IS 13252
Environment
IEC 60068-2-1, IEC 60068-2-2, IEC 60068-2-14
IEC 60068-2-6 (vibration), IEC 60068-2-27 (shock), IEC 60068–2–30, IEC 60068-2-78, IEC/EN 60529 IP52, IEC/EN 62262 IK08
Network
NIST SP500-267
Dimensions
Height: 101 mm (4 in)
ø 149 mm (5 7/8 in)
Weight
550 g (1.2 lb)
Languages
English, German, French, Spanish, Italian, Russian, Simplified Chinese, Japanese, Korean, Portuguese, Traditional Chinese
Warranty
5-year warranty