AXIS A4020-E Reader
Designed to perfectly match network door controllers and credentials from the manufacturer, the reader offers secure and seamless touch-free entry. Ideal for use in harsh environments both indoors and outdoors, it features a mullion-mount design to fit perfectly in narrow spaces and door frame installations. It supports most types of smart RFID card standards with 13.56MHz credential technologies and includes out-of-the-box support for Open Supervised Device Protocol (OSDP) for secure bidirectional communication. Packed with built-in cybersecurity features, it helps prevent unauthorized access and safeguards your system. Furthermore, this smart reader supports Secure Channel Protocol (SCP) enabling secure communications and connections.
• Designed to perfectly match manufacturer’s door controllers and credentials
• Support for most RFID cards with 13.56MHz
• IP65, IK07 ratings for use in harsh environments 
• EAL6+ Certified Secure Element for added protection 
• Mullion-mount design for easy installation

The manufacturer shall provide free upgrades to new software releases within the same major version for the lifetime of the version.
The embedded analytics shall be backed by free support within warranty period.
The contractor or designated subcontractor shall submit credentials of completed manufacturer certification, verified by a third party organization, as proof of the knowledge.
The main unit shall be manufactured by a company that have signed and support the UN Global Compact initiative as defined by United Nations www.unglobalcompact.org/

Reader technology
13.56 MHz ISO14443A and ISO14443B (MIFARE Classic®, MIFARE Plus® (Level 1), MIFARE DESFire® EV1, EV2, and EV3).
Network protocols
Open supervised device protocol (OSDP)
Alarm status indication
RGB LED for user feedback, buzzer
Detection type
Built-in tamper switch for detecting both open casing and removal from wall
Edge security
Hardware: cryptographic compute module cybersecurity platform
Secure element (CC EAL 6+), secure keystore, secure boot
Casing
IP65 and NEMA 4X-rated, IK07 plastic casing, hard-coated scratch- and impact-resistant front
Color: black NCS S 9000-N
Mounting
Suitable for mullion-mount door installations or any flat surface mounting
Security
EAL 6+ Certified Secure Element Hardware
Power
Input: 12 V DC
Current consumption: Typical 60 mA@12 V, peak 100 mA@12 V
H-field strength = 15.63 dBμA/m @3m
Connectors
4-pin 26–18 AWG terminal block for RS485 (A/B) and power (+/-)
Cable requirements
Power: 26–18 AWG (0.13–0.82 mm2)
Reader data: 1 twisted pair with shield, 26–18 AWG (0.13–0.82 mm2), 120 ohm impedance, for A and B. Qualified for up to 1000 m (3281 ft) – 24 AWG.
Operating conditions
-40 °C to 65 °C (-40 °F to 149 °F)
Humidity 10–100% RH (condensing)
Storage conditions
-40 °C to 65 °C (-40 °F to 149 °F)
Humidity 5–95% RH (non-condensing)
Approvals
EMC
EN 61000-6-1, EN 61000-6-3, FCC Part 15 Subpart B Class B
Wireless
EN 300330, EN 301489-1, EN 301489-3, EN 62311, FCC Part 15 Subpart C
Safety
CAN/CSA-C22.2 No. 60950-22, CAN/CSA C22.2 No. 62368-1, IEC/EN/UL 60950-22, IEC/EN/UL 62368-1, UL 294
Environment
IEC 60068-2-1, IEC 60068-2-2, IEC 60068-2-6, IEC 60068-2-14, IEC 60068-2-27, IEC 60068-2-78, IEC/EN 60529 IP66, IEC/EN 62262 IK07, NEMA 250 Type 4X
Dimensions
121 x 48 x 27 mm (4.76 x 1.89 x 1.06 in)
Weight
118 g (4.16 oz)
Warranty
5-year warranty