AXIS Q6358-LE PTZ Camera
This product features an outstanding light-sensitive ½” inch sensor, 31x optical zoom, laser focus and quick zoom. Built on a chipset (9th gen), it offers accelerated performance to run impressive analytics applications on the edge. For instance, object analytics can detect and classify humans, vehicles, and types of vehicles. This IP66-, IK10-, and NEMA 4x-rated device is impact- and weather-resistant. Plus, it’s NEMA TS2 rated so it can be used in temperatures up to 74°C. Reduced bandwidth and storage needs with support for AV1, H.264, and H.265 significantly lowers bandwidth and storage requirements. Furthermore, cryptographic compute module safeguards your device and protects sensitive information from unauthorized access.
• 1/2" sensor with 31x optical zoom
• advanced WDR imaging technology, low-light technology, and IR
• Next-generation AI-powered analytics
• Reduced bandwidth and storage needs with AV1, H.264, H.265
• Built-in cybersecurity with cryptographic compute module

Image sensor
1/2” progressive scan CMOS
Lens
Optical zoom: 31x
Zoom speed: <1 sec between any zoom value
Focal length: 6.91 – 214.64 mm
Horizontal field of view: 60.6°– 2.0°
Vertical field of view: 36.5°– 1.1°
Laser focus, autofocus, P-iris
Day and night
Automatically removable infrared-cut filter
Minimum illumination
Color: 0.1 lux at 30 IRE, F1.36
B/W: 0.005 lux at 30 IRE, F1.36, 0 lux with IR illumination on
Color: 0.2 lux at 50 IRE, F1.36
B/W: 0.009 lux at 50 IRE, F1.36, 0 lux with IR illumination on
Shutter speed
1/111000 s to 1/2 s
Pan/Tilt/Zoom
Pan: 360° endless, 0.05°– 550°/s
Tilt: +20 to -90°, 0.05°– 500°/s
Zoom: 31x optical, 12x digital, Total 372x zoom
Quick-zoom, nadir flip, 300 preset positions, tour recording (max 10, max duration 16 minutes each), guard tour (max 100), control queue, on-screen directional indicator, set new pan 0°, adjustable zoom speed, advanced dome cleaning function
System on Chip model
Manufacturer’s own chipset (9th gen)
Memory
4096 MB RAM, 8192 MB Flash
Compute capabilities
Deep learning processing unit (DLPU)
Video compression
AV1
H.264 (MPEG-4 Part 10/AVC) Baseline, Main and High Profiles
H.265 (MPEG-H Part 2/HEVC) Main Profile
Motion JPEG
Resolution
3840x2160 4K UHD
Frame rate
Up to 50/60 fps (50/60 Hz) in all resolutions
Video streaming
Multiple, individually configurable streams in AV1, H.264, H.265 and Motion JPEG
Reduced bandwidth and storage needs technology in AV1, H.264 and H.265
Controllable frame rate and bandwidth
VBR/ABR/MBR AV1/H.264/H.265
Low latency mode
Video streaming indicator
Signal-to-noise ratio
>55 dB
Image settings
Compression, color, brightness, sharpness, white balance, exposure control, exposure zones, image freeze on PTZ, scene profiles, rotation, electronic image stabilization (EIS), defogging
Contrast, local contrast, autofocus, advanced WDR imaging technology: Up to 120 dB depending on scene, 100 individual polygon privacy masks including mosaic and chameleon privacy masks
Audio input
Input through portcast technology
Audio output
Output through portcast technology
Network protocols
IPv4, IPv6 USGv6, ICMPv4/ICMPv6, HTTP, HTTPS, HTTP/2, TLS, QoS Layer 3 DiffServ, FTP, SFTP, CIFS/SMB, SMTP, mDNS (Bonjour), UPnP®, SNMP v1/v2c/v3 (MIB-II), DNS/DNSv6, DDNS, NTP, NTS, RTSP, RTCP, RTP, SRTP/RTSPS, TCP, UDP, IGMPv1/v2/v3, DHCPv4/v6, ARP, SSH, NTCIP, LLDP, CDP, MQTT v3.1.1, Secure syslog (RFC 3164/5424, UDP/TCP/TLS), Link-Local address (ZeroConf)
Application Programming Interface
Open API for software integration

ONVIF® Profile G, ONVIF® Profile M, ONVIF® Profile S, and ONVIF® Profile T, specification at onvif.org
Onscreen controls
IR illumination
Quick-zoom
advanced dome cleaning function
Event conditions
Device status: above operating temperature, above or below operating temperature, below operating temperature, fan failure, IP address removed, IP address blocked, live stream active, network lost, new IP address, PTZ power failure, system ready, within operating temperature
Edge storage: recording ongoing, storage disruption, storage health issues detected
I/O: manual trigger, virtual input
MQTT: MQTT client connected
PTZ: PTZ malfunctioning, PTZ movement, PTZ preset position reached, PTZ ready
Scheduled and recurring: schedule
Video: average bitrate degradation, day-night mode
Event actions
Day-night mode: Use day-night mode while the rule is active
Defog: set defog mode, set defog mode while the rule is active
Illumination: use lights, use lights while the rule is active
Images: FTP, SFTP, HTTP, HTTPS, network share and email
MQTT: MQTT publish
Notification: email, HTTP, HTTPS, TCP
Overlay text: use overlay text, use overlay text while the rule is active
Recordings: record video, record video while the rule is active
Security: erase configuration
SNMP: trap messages, trap messages while the rule is active
Video clips: FTP, HTTP, HTTPS, SFTP, email, network share
Applications
Included
object analytics, scene metadata, video motion detection, OSDI Zone, Orientation Aid PTZ, advanced gatekeeper, autotracking 2
Supported
Object Analytics
Object classes: humans, vehicles (types: cars, buses, trucks, bikes, other)
Scenarios: line crossing, object in area, time in area, crossline counting, tailgating detection, PPE monitoringBETA, motion in area, motion line crossing
Up to 10 scenarios
Other features: triggered objects visualized with trajectories, color-coded bounding boxes and tables
Polygon include/exclude areas
Perspective configuration
ONVIF Motion Alarm event
Scene metadata
Object classes: humans, faces, vehicles (types: cars, buses, trucks, bikes), license plates
Object attributes: vehicle color, upper/lower clothing color, confidence, position
EMC
EN 55032 Class A, EN 55035, EN 61000-3-2, EN 61000-3-3, EN 61000-6-1, EN 61000-6-2, CISPR 35, EAC, EN 50121-4
Australia/New Zealand: RCM AS/NZS CISPR 32 Class A
Canada: ICES-3(A)/NMB-3(A)
Japan: VCCI Class A
Korea: KS C 9835, KS C 9832 Class A
USA: FCC Part 15 Subpart B Class A
Railway: IEC 62236-4
Safety
IEC/EN/UL 62368-1, CAN/CSA C22.2 No. 62368-1, IEC/EN 62471 risk group 2, IEC 60825-1 Class 1
Environment
IEC/EN 62262 IK10, IEC/EN 60529 IP66, IEC/EN 60529 IP67, NEMA 250, Type 4X, NEMA TS 2 (2.2.7–2.2.9), IEC 60068-2-1, IEC 60068-2-2, IEC 60068-2-6, IEC 60068-2-14, IEC 60068-2-27, IEC 60068-2-78, ISO 21207 (Method B), ISO 12944-6 C5
Network
NIST SP500-267
Cybersecurity
ETSI EN 303 645, BSI IT Security Label, FIPS 140
Edge security
Software: Signed OS, brute force delay protection, digest authentication and OAuth 2.0 RFC6749 Client Credential Flow/OpenID Authorization Code Flow for centralized ADFS account management, password protection, AES-XTS-Plain64 256bit SD card encryption
Hardware: cryptographic compute module cybersecurity platform
Secure keystore: secure element (CC EAL6+, FIPS 140-3 Level 3), system-on-chip security (TEE)
Manufacturer's device ID, signed video, secure boot, encrypted filesystem (AES-XTS-Plain64 256bit)
Network security
IEEE 802.1X (EAP-TLS, PEAP-MSCHAPv2), IEEE 802.1AE (MACsec PSK/EAP-TLS), HTTPS/HSTS, TLS v1.2/v1.3, Network Time Security (NTS), X.509 Certificate PKI, host-based firewall
Casing
IP66-, IP67-, NEMA 4X- and IK10-rated
Color: white NCS S 1002-B
Repaintable metal casing (aluminum), hard coated Polycarbonate (PC) clear dome with innovative dome rotation technology technology
Power
IEEE802.3bt Type 3 Class 6
Possibility to optimize power consumption of camera:
Full power: typical 13.7 W (no IR), max 51 W
Low power: typical 13.7 W (no IR), max 30 W. With IR: 40 W
Features: power profiles, power meter
Connectors
RJ45 10BASE-T/100BASE-TX/1000BASE-T
RJ45 Push-pull Connector (IP66)
Audio: Audio and I/O connectivity via portcast technology
IR illumination
IR with power-efficient, long-life 850 nm IR LEDs
Range of reach 300 m (984 ft) or more depending on the scene
Storage
Support for SD/SDHC/SDXC card
Support for SD card encryption (AES-XTS-Plain64 256bit)
Support for recording to network-attached storage (NAS)
For SD card and NAS recommendations, refer to the manufacturer's webpage
Operating conditions
Full power: -50 °C to 55 °C (-58 °F to 131 °F)
Low power: -10 °C to 55 °C (14 °F to 131 °F)
Maximum temperature according to NEMA TS 2 (2.2.7): 74 °C (165 °F)
intelligent camera heating technology: Start-up as low as -40 °C (-40 °F)
Humidity 10–100% RH (condensing)
Storage conditions
-40 °C to 65 °C (-40 °F to 149 °F)
Humidity 5-95% RH (non-condensing)
Dimensions
Height: 261 mm (10.3 in)
With weather shield: ø 239 mm (9.4 in)
Without weather shield: ø 192 mm (7.6 in)
Weight
4 400 g (9.7 lb)
Languages
English, German, French, Spanish, Italian, Russian, Simplified Chinese, Japanese, Korean, Portuguese, Polish, Traditional Chinese, Dutch, Czech, Swedish, Finnish, Turkish, Thai, Vietnamese
Warranty
5-year warranty
Substance control
PVC free, BFR/CFR free in accordance with JEDEC/ECA Standard JS709
RoHS in accordance with EU RoHS Directive 2011/65/EU and 2015/863, and standard EN IEC 63000:2018
REACH in accordance with (EC) No 1907/2006. For SCIP UUID, see echa.europa.eu
Materials
Renewable carbon-based plastic content: 23% (recycled: 18%, bio-based: 5%, carbon capture based: 0%)
Screened for conflict minerals in accordance with OECD guidelines
Environmental responsibility

The manufacturer is a signatory of the UN Global Compact, read more at unglobalcompact.org